<?xml version="1.0"?>

<definition>

  <config model="Chicony KBP-8993 keyboard">
  <!--
          Contributed by Matthijs Melchior <mmelchio@xs4all.nl>
          The extra keys need to be enabled by sending the bytes 0xea and 0x71
          to port 0x60 using the standard keyboard protocol.
          I do this using the kbd_cmd program available in the source package `kbd'.
  -->
  
    <PrevTrack    keycode="163"/>
    <Play         keycode="162"/>
    <Stop         keycode="164"/>
    <NextTrack    keycode="161"/>
  
    <VolUp        keycode="153" adj="2"/>
    <VolDown      keycode="146" adj="2"/>
    <Mute         keycode="160"/>
  
    <WebBrowser   keycode="178"/>
    <Shell        keycode="176"/>
    <MyDocuments  keycode="151"/>
    <Sleep        keycode="165"/>
  
    <userdef keycode="174" command="gnome-terminal --use-factory --start-factory-server">Close</userdef>
    <userdef keycode="158" command="gnome-terminal --use-factory --start-factory-server">zzZ</userdef>
    <userdef keycode="166" command="gnome-terminal --use-factory --start-factory-server">Menu</userdef>
  
  
  </config>

  <contributor>
    <name>to be added</name>
    <email>to be added</email>
  </contributor>

</definition>
